(module usb (layer F.Cu) (tedit 5CAA3F4B)
  (fp_text reference REF** (at 0 6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value usb (at 0 -2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4 -1) (end 4 -1) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 -1) (end 4 5) (layer F.SilkS) (width 0.12))
  (fp_line (start 4 5) (end -4 5) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 5) (end -4 -1) (layer F.SilkS) (width 0.12))
  (pad 1 smd rect (at -1.3 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.65 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.65 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.3 0) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 3.1 0.125) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -3.1 0.125) (size 2.1 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.2 2.675) (size 2.15 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.2 2.675) (size 2.15 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 3.8 2.675) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -3.8 2.675) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask))
)
