(module XKB5858-Z-TP (layer F.Cu) (tedit 5DACA2AC)
  (fp_text reference REF** (at 0 4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value XKB5858-Z-TP (at 0 -4) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3 -3) (end 3 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 -3) (end 3 3) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 3) (end -3 3) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 3) (end -3 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 1.5) (end -1.5 -1.5) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -3.375 -2) (size 2.55 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.375 0) (size 2.55 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -3.375 2) (size 2.55 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 3.375 -2) (size 2.55 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 3.375 0) (size 2.55 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 3.375 2) (size 2.55 0.8) (layers F.Cu F.Paste F.Mask))
  (model ${KIPRJMOD}/audioMux.pretty/XKB5858-X-TP.step
    (offset (xyz 0 0 5.5))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
