(module "XKB_X05B20U04T" (layer F.Cu) (tedit 5DF58751)
  (fp_text reference "REF**" (at 0 7 unlocked) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "XKB_X05B20U04T" (at 0 -1.6 unlocked) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.8 5.9) (end -3.8 5.9) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.8 5.9) (end -3.8 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.8 0) (end 3.8 5.9) (layer F.SilkS) (width 0.12))
  (pad "1" smd rect (at -0.75 0) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -0.25 0) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 0.25 0) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 0.75 0) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "MNT" smd rect (at -2.4 2.35) (size 2 3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "MNT" smd rect (at 2.4 2.35) (size 2 3) (layers "F.Cu" "F.Paste" "F.Mask"))
)
